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附圖一：系爭專利主要圖式
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附圖二：系爭產品「夜行者」電競鍵盤照片
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附圖三：引證1第1圖
[image: 引證1]

附圖四：引證2第五圖（第二具體實施例）
[image: 引證2]

附圖五：引證4圖2
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附圖六：系爭產品按鍵的定義（見原告所提103 年11月24日民事準備狀附件十六）
	Item Tag (Value)
	Raw Data

	Usage Page (Generic Desktop)
	05 01

	Usage (Keyboard)
	09 06

	Collection (Application)
	A1 01

	Report ID (3)
	85 03

	Report Count (56)
	95 38

	Report Size (1)
	75 01

	Logical Minimum (0)
	15 00

	Logical Maximum (1)
	25 01

	Usage Page (Keyboard/Keypad)
	05 07

	Usage Minimum (Keyboard Left Control)
	19 E0

	Usage Maximum (Keyboard Right Control)
	29 E7

	Usage Minimum (Undefined)
	19 00

	Usage Maximum (Keyboard [ and {)
	29 2F

	Input (Data,Var,Abs,NWrp,Lin,Pref,NNul,Bit)
	81 02

	End Collection
	C0

	Usage Page (Generic Desktop)
	05 01

	Usage (Keyboard)
	09 06

	Collection (Application)
	A1 01

	Report ID (4)
	85 04

	Report Count (56)
	95 38

	Report Size (1)
	75 01

	Logical Minimum (0)
	15 00

	Logical Maximum (1)
	25 01

	Usage Page (Keyboard/Keypad)
	05 07

	Usage Minimum (Keyboard ] and })
	19 30

	Usage Maximum (Keyboard =)
	29 67

	Input (Data,Var,Abs,NWrp,Lin,Pref,NNul,Bit)
	81 02

	End Collection
	C0








附圖七：原告所提陳報（三）狀附件八同時按壓1、2、3、4、Q、W、E、A、S、D等10個按鍵時，測試程式收到「03 00 90 01 50 C4 03 00」，其中第一個「03」為Report ID。
	按鍵
	ID
	Byte 2
	Byte 3
	Byte 4
	Byte 5
	Byte 6
	Byte 7
	Byte 8

	1
	03
	00000000
	00000000
	00000000
	00000000
	01000000
	00000000
	00000000

	2
	03
	00000000
	00000000
	00000000
	00000000
	10000000
	00000000
	00000000

	3
	03
	00000000
	00000000
	00000000
	00000000
	00000000
	00000001
	00000000

	4
	03
	00000000
	00000000
	00000000
	00000000
	00000000
	00000010
	00000000

	Q
	03
	00000000
	00000000
	00000000
	00010000
	00000000
	00000000
	00000000

	W
	03
	00000000
	00000000
	00000000
	00000000
	00000100
	00000000
	00000000

	E
	03
	00000000
	00000000
	00000001
	00000000
	00000000
	00000000
	00000000

	A
	03
	00000000
	00010000
	00000000
	00000000
	00000000
	00000000
	00000000

	S
	03
	00000000
	00000000
	00000000
	01000000
	00000000
	00000000
	00000000

	D
	03
	00000000
	10000000
	00000000
	00000000
	00000000
	00000000
	00000000

	輸出
	03
	00000000
	10010000
	00000001
	01010000
	11000100
	00000011
	00000000

	
	03
	00
	90
	01
	50
	C4
	03
	00







6

image5.png
[EIfL e
1R Y N Y Y Y A O R Y ¢ ¢ M M

2

S

firrfiAR

VI d e





image6.png
/1 04
2 S VEDZS|

R AR

B sand VETFS
— S

: ALTY-

SHIFT(R) : ASHIFTX-
CTRL(R) : &CIRLY~

Yo Y ¥z Y3
ALT |SHIFT| CTRL | ENT
Xg
R ® | ®
ALT (SHIFT| CTRL | ENT
X
w | W w | w
Xa | ! 2 3 4
X3 | & 6 7 M
ALT(L) : ZEALT%- ALT(R)
SHIFT(L) : ZESHIRTH-
CTRL(L) : ZZCIRLA-
ENT : 47" HRENTER—
ENT (T) : #/4%-#BENTER%-




image1.png
X10

X11

X12

X13

X14

X15

YO0 Y2 Y3 Y4 Y5 Y6 Y7

Fllp Pre Next Message
track track Webcam |[status

Photo
Gallery| Vol+ Vol- Refresh | Ctrl-R | Message
wWwWw
Back ALT-L Forward | stop
WwWw N-CHG CHG
Win-L Home (K131) (K132) (K133)
KOR1 KOR2
Caculator| Sleep (K150) (K151)
{
[

}
]

Print
Space F11 Screen Home - Delete
Scroll
F12 Lock
I
|
ﬁ 7
(pad)
/ 8
o | <2 | G
X 9
- + K107 Enter
(pad) | (pad) (pad) (pad)

Play / Media Media Media
Lock Pause Select | Shift-R| Mute Stop

gl
T

£
(—F
®
]
Fl o+ - e | —
O
P =
=
N
(=2]

Esc

-ry
83
H
—~ =
%gg

QO

a

-

-ry
NN
I=a]
ok
=N

EE

5E

~x3 ~xy -y
< (=) -3

Insert

l\’)

g’_
N

d

B

{8‘\05 N QA O | OO 3| =]
s E
o/ o/ N/

E (B
~r (>

pal

ORRR: PRRPPPEE
EEE@IIIEE




image2.png
ASharkoen
P &

eS| =

RTINS  <KEYBORRD

(L EFE S

o
FeRTURES
= SERRESsERES

= 20 B% R aER

= 8 BAHARRIBRILRE B izaTo

= SHEHBRUREAEATROEH LR A
(#): Photoshop, Windows, 58 %)

= Xif 18 RFEHR

u SERRTEX LR { ERE)

= SHESERRESLE 10 GRER Bloven 0




image3.png
8 BARRARBHRAR

Juss
I
—FEE
oC.as0C
azcosssC
aEpmse:

= RIS R REBERNER
(f¥: Photoshop, Windows, SERS %)

= i 18 RFHR

= SERRTER LR

= ERAVTDEARELE 10 AIREHE

= WER RN ER. AE. SRMNAE.
AAPEREThRE. AR, REIDAE. EERME

BENZDH:

= SKILLER TR EHAS KBRS
= 8 MRS HATRYRRR

= AR K REAF R (PDF 1)

R
x\\\ *““ \\

3 AN
v \\\\§§<\\\ \f\\
ey

SENE: 10
R+:512 x 330 x 225 mm
4044951101243

~1
RE: vE

O BRI www.sharkoon.com
ohl FiE AP FmiE BRADS BESERE IR




image4.png
RETR

0 1 2 3 4 5 5 7
i (132) ¥(14) | \[2942) | App (126) Del(76)
2 (13 | Z46) [ AGY)___|Qi7) 102 |ESC(i10)
3 S(89) W(ig) (9 | 1(83) | End43) | Fi2(123) | Num(S0) | Ins(75)
4 Spe6l)__ | 1(84) 128 [ [27) | BKkSp(i5) | Fi0(i21) | =(13) _|Fii(122)
5 Win
6 Altf60)
7 ) No.56(56) 55 |40) | P@e. [P0 |12 loq1)
AR g 54 LU /0@ [Fri18)_ |o0) _ [Fe(i19)
9 M52) NG1) I3 6(07) uEs)__ [708)
10 B(50) FB)77] Giss) | T@21) [ 4(05) R(20)__|5(06)
1 Rshitt57) Lshift(44)
12 Kana (133) L EZI) Fo(i17) | 809 _ |F5(118)
13 RCIr(64) LCtr(58)
14 C{48) [ DBA)Z E(9)_ |F3(i14) | 304 [F4(15)
15 01) X4 1539 F2(113) [ 203) _ [Fi(i12)
\ 16 Vid9) Fn Caps(30) | Tab(16) | H(36) Y@2)





