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NOTES:
1MOUNTING PANEL THICKNESS 3.5mm MAX
13 27THE PRODUCT IS ROHS COMPUANT

ELECTRIAL PERFORMANCE:
| 1IMPEDANCE:50 Ohms
| 2 FREQUENCY:DC~8GHz
3NSULATOR RESISTANCE:DCSOV>10000M Onms.

.| SIMPULSE DISCHARGE VOLTAGE:SKY min

- 5.0PERATION AND STORAGE TEMPERATURE:-40°C~90°C

NUT EYSWR20:1 Mox
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