附圖1（系爭專利主要圖面）
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附圖2
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[image: image5.jpg][0061] The rotor 14 has a passage 18 provided therein for
communication with the fixed tube 12. The fixed tube 12 and
the rotor 14 are joined to each other rotatably and airtightly,
whereby the pressurized air derived from the pressurized gas
source 50 through the fixed tube 12 can be conveyed through
the passage 18 to be ejected from a nozzle tip 15.







