108行專訴字第84號判決附圖
附圖一、系爭專利主要圖式
[image: ]
        管接頭分解圖
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                       接頭螺件與緊束環之分解圖
[image: ]
 組合剖視圖暨局部放大示意圖
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            剖切實物照片如下：
[image: ]

[image: ]統一發票如下方所示，其中一張發票日期為102年11月18日，品名為「0122028 LFPB9604-CP 1/4」；另一張發票為「成毓有限公司」於102年12月10日開立給「夷帝企業有限公司」，品名為「0122028 LFPB9604-CP 1/4」。
[image: ]

標籤如下方所示，記載品名為「0122028 LFPB9604-CP 1/4」。
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[image: ]出口報單影本如下方所示，記載夷帝企業有限公司於102年12月17日報關，貨物名稱「0122028 LFPB9604-CP 1/4」，數量為「9600」。









附圖三、證據3主要圖式
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附圖四、證據4主要圖式
[image: ]
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[image: ]附圖五、證據5主要圖式
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WWATTS® LFPB9604

Compression >
Saddle Valve 1/4in OD

Robinet-valve & étrier Qty: 100
Valvula de montaie 0122028

*LEAD FREE: Tho wetted surtace of this product contacted by
consumable water contains less than 0.25% of lead by weight.

“SANS PLOMB: Los surfaces de ce produlten contact avec
eau potable contiennent mains de 0.25 % de plomb par poids.

e bl d 2 00 98268 70661 5

0.25% de plomo por peso. Made in Taiwan/Fabrique en Taiwan/Hecho en Taiwan
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Installation Instructions:

1. Assemblg own in figure (1), with piercing pin
retractod ly the w (kg by mgnnn( o valvt handi "
counter-clockwise, Caution: be sure the piercing pin does not
protrude down beyond the top clamp.

2. With th (8) in fixed position, clamp the entire
:mmh.fy“mlry‘:uw v(m)ur supplg line using mg bolts, nuts,
and base clamp provided.

3. Comple Inection to the valve outlet, For 1/4” 0D
pnlygmm m.o.;-o :nlylnnyhm, the insert and nut with captive
sleeve should be used as shown, For 1/4” 0D copper tul ||P the
Insert only should be removed. Tubing should be inserted fully
%mh mn' nut and attached to the valve at a 45° angle. Wrench

4. mwﬁ the handle clockwise to pierce the supply line and close the
5. "Ignpen valve, turn handle counter-clockwise to desired water
w.

Instrucciones de instalacion:

T fcemo o vl tl com se muestraen (1), co fpesado e perfracon el
e ers sparr gt o manid vl il it Pricauoin ssgirse
b e ol pasador do prfracén 1o soextienda haci abao mds all de 1 abrazaners Supriy

2 Ganlajnta de goma 3 en psiln s e todo o montlefimemente alconductodo suminsro o
‘oua oo os pemos, 6 tercas y I abrazadera e base que sa proporcionan:

- Gamplete i conexio a i ad o vélvula, n s tubrfas d poletieno o polbutieno ds 0,64 (1/4
de g, da démetroextemo, ol aceasoroy I uerca con f Cauio deben usarso bl como oo
uesira. En as uborasde oobre de 0,64 o 1/4 e pug,) da clmetro xtemo, o au

nicaments ol accosario La tuberia ebe insenarse complatamants a evss e a tuercay conpelarss
valvlaa un énouo e 45°. Aprete s terca con una leve,

3. Gite i manif haca a derecha parapertorar o conductodo suminitro y cere la vl

©Paraabi la vivula, giro Ja manja heca I zquirt hasia aicanzar e o g6 agua dsoaco

A/ARNING: Tis poductcotanechamicals Khown o te tats of Calforia o cause cancerand bt
eectsor oer reprouctve harm. For mora information ww.watt.com/prapgs

ADVERTENGIA: Ete producto confiene quinicos que el Estado Catoma onsdra e s ey
fectos do nackinio ufrs daos durnt agestaco.Pars s BT st o

m 1503 @
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